RX12 Changelog

# Firmware

Version 1.0 – First tested and flown version.

Version 1.01

* If receiver is powered on before transmitter the log will no longer show a Failsafe alert.

Version 1.2

* Added PPM output option on Ch. 12 pins.

Version 1.3

* Added SBus output option on Ch. 12 pins.
* Changed blink codes to make them easier to distinguish.

Version 1.4

* Changed PPM output order to AETR to maintain compatibility with PPM encoders.
* Fixed SBus bug – Throttle channel was incorrect.
* SBus failsafe bit was in wrong position.

Version 1.5

* PWM outputs 1-11 are now active even in SBus mode. Output 12 is used for SBus so channel 12 is not available in PWM format.

# Client

Version 1.00 – Initial version

Version 1.1 – Added PPM option

Version 1.2 – Added S.Bus option

Version 1.3 – Changed connection behavior. Now only reports “Connected” after successful read. Now Save button is only enabled after successful read.

# Schematic and PCB

Version 1.0 – Initial production version