RX12 Changelog

# Firmware

Version 1.0 – First tested and flown version

Version 1.01

* If receiver is powered on before transmitter the log will no longer show a Failsafe alert.

Version 1.2

* Added PPM output option on Ch. 12 pins

Version 1.3

* Added S.Bus output option on Ch. 12 pins
* Changed blink codes to make them easier to distinguish

Version 1.4

* Changed PPM output order to AETR to maintain compatibility with PPM encoders
* Fixed SBus bug – Throttle channel was incorrect
* SBus failsafe bit was in wrong position.

# Client

Version 1.00 – Initial version

Version 1.1 – Added PPM option

Version 1.2 – Added S.Bus option

# Schematic and PCB

Version 1.0 – Initial production version