RX12 Changelog

# Firmware

Version 1.00 – First tested and flown version

Version 1.01

* If receiver is powered on before transmitter the log will no longer show a Failsafe alert.

# Client

Version 1.00 – Initial version

# Schematic and PCB

Version 1.0 – Initial production version